
Driver-specific options:
(To be set in the config file by parameter 'bs' under section 'bus'.)

    rpanic=num      Defines read panic threshold (default: 48)
    tpanic=num      Defines write panic threshold (default: 16)
